Studio
Studio dimensions: 53’x31’ (1650 Sq Ft)
[image: ]


Chroma Green Cyc: L shaped 29'-6" x18'-6" x 11’-4”
Curtains
4 panels of 18’ X 40’ Black
4 panels of 18’ X 40’ White
Lighting
Lighting console: ETC Element 2
Instruments
10 Lumos Hawk 150 3200K
25 Lumos Hawk 200 3200K
10 Chroma-Q Space Force one by two Bicolor
10 Altman Spectra CYC 100 3200K
8 ETC S4wrd Color II LED retro fit RGBA, Source 4 body
2 ETC S4wrd 90 CRI 3200K retrofits, Source 4 body
Grip
Grip: Swivel Clamps, Side arms, pipe Battans
Cameras
3 Sony HDC3500 on Ross Furio Cambots
1 Sony HDC3500 On a 12’ jib arm
AutoScript Teleprompter
Audio
8 Wisycom MTP40S wireless beltpack tranmiters, with 16 Countryman Associates B3W4FF05BS3 lavalier microphones
1 Wisycom MTH410-USX Wireless Handheld Transmitter with Wisycom MCM306 Supercardiod condenser Capsule
4 Wisycom MPR50-IFB wireless IFB receivers with Bumblebee industries Earpeices
64 analog audio inputs via a Dante audio network
Control Room:
Video Switcher: Ross 3 M/E Acuity with 3D DVE
Audio Console: Yamaha QL5 Mixer
Graphics: Ross Xpression Studio 12
Virtual Set: Ross Voyager - virtual set technology, 3 Cameras trackless
Communications / talkback: RTS Intercom with RTS wireless Belt pack
Transmission capabilities
Connected for Receive and Transmit to The Switch at 60 Hudson
East and West coast satellite uplink and downlink
AWS Elemental Encoder for outbound streaming encodes
Harmonic XOS for inbound streaming decodes
Cloud-based Iconik MAM and Sony Ci for secure file based send and receive
Connectivity
Dual diverse 10 Gbps data links
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